Fevicol marine is specially designed for bonding in Furnitures, which is exposed to water or placed in high humidity areas. 1 hour boiling water resistance, superior bonding in marine plywood, higher coverage, applications, for bonding wood, plywood, laminates, veneers, partical board, block board/hard board, mdf to each other, kitchen units, wall units, bathroom where exposure to water is high, pencil mfg.

Fevicol Probond is a specialised adhesive for pasting PVC Sheets, Acrylic Sheets and primer coated edge banding tapes on wood and plywood surfaces. It needs to be applied on only one surface for pasting PVC edge banding tapes and on both the surfaces for pasting Acrylic or PVC laminate sheets

FEVICOL SR998 is a synthetic rubber based solvent containing contact adhesive specially designed for Industrial segment. It exhibits excellent bonding strength. The adhesive dries to a tough, flexible film with good resistance to water and aging. This adhesive can be applied by brush, or roller coater. SALIENT FEATURES : Free from Benzene- Non-hazardous to health. Excellent Strength. Preferred by the users dealing only in quality works.

Fevicol SH is a synthetic Adhesive in the form of a milky white viscous paste and is ready to use. Fevicol SH gives very strong bond. The bond is so strong that if two wooden pieces are joined with Fevicol SH and a hammer is hit heavily, the wood will give way but not the fevicol bond. Resistance to water & heat, economical in long run, gives higher coverage, applications, for bonding wood, plywood, laminates, veneers, partical board, block board/hard board, mdf to each other, pencil mfg. Sports goods, paper, carpet mfg.

Introducing Fevicol SR 505, specially for PVC flooring, foam/rexine upholstery Fevicol SR 505 is free from harmful benzene

Fevicol HeatX is a synthetic solvent borne rubber based adhesive made with a special formula for having excellent heat resistance property up-to 170Â°C temperature. Fevicol HeatX is having Excellent heat resistance

Superfast and convenient way to paste laminate (paper laminates/PVC laminates) to plywood. Fevicol Ezeespray is a spray adhesive that allows even a layman to paste small to medium sized laminates to plywood within 10 minutes. Now, why wait for contractors to do small jobs/repairs when you can do it yourself. Handling and storage 1. Do not expose to temperatures exceeding 50°c 2. Avoid exposure to direct sunlight 3. Do not store directly on the concrete floor

Introducing Fevicol Foamfix with faster bonding to your expectation. Specially for making superior quality sofa, chair, mattresses etc. Fevicol Foamfix is free from harmful Benzene.

Fevicol Speedx Synthetic Resin Adhesive for the first time in india, a revolutionary adhesive which can save time and increase productivity.

Fevicol Hi-Per powered with Anti-Bubble formula provides instant grab and uniform glue transfer leading to a strong contact between plywood & laminate.

Hence there is a very little chance of air entrapment and contact gap which significantly reduces the probability of bubble formation. It also offers superior tack development, faster grab and reduced setting time

**Fevicol HeatX is the future of all lamination jobs. It is a new age adhesive which is incomparable to any other adhesive in the market**

**FEVICOL** **XPRESS** 1000 heat shield is a synthetic solvent borne rubber basedadhesive which is resistant to water. ... We are fully geared to offer the consumer world class products that give optimum value for their investment which provide the consumer a truly international living environment

**Fevicol a- kwik** grab is a high strength multipurpose adhesive to bond almost all materials. Gives instant grab and forms a long lasting elastic bond.

**Marinekoat is a far more economic and simpler solution compared to conventional options like backside lamination or bison board panelling**

**Fevicol 707 FW** from the house of **Pidilite**. The offered product is a synthetic rubber adhesive, which is commonly used in footwear industry.

Woodggrip super is used For bonding wood,plywood,laminates,veneers,particle board,block board/hard board,MDF to each other. Pencil mfg,sport goods,paper labeling,paper tube,wall paper,carpet mfg.

Woodgrip marine is a Synthetic Rubber Based Adhesive may be used interchangeably with glue, cement, mucilage, or paste, and is any substance applied to one surface, or both surfaces, of two separate items that binds them together and resists their separation.Adhesives are typically organized by the method of adhesion.

Wood Grip ms1 is a high viscosity adhesive with an advantage of better grab. Because of its unique "WOODGRIP WITH A TIGHT GRIP" feature grip remain till the end.

This product is Pidilite Fevitite Repid, 36g. It is used in art purpose . Fevitite rapid is a two-component multipurpose epoxy adhesive

Fevitite Super strong is a two component fast setting super strength epoxy adhesive that bond virtually anything to anything in 2-3 hours.

Grippo is a revolutionary adhesive which can save time and increase productivity.

Bullbond lc is a white viscous paste used for its features like Versatility, hearth resistance, shock and vibration resistance, Non-staining etc.